BluePhone

- version - myLink - myConvert - m_Port - m_Device - m_BtAddress - m_BtChannel - m_BtChannelInt - m_ConnectStartup - m_phoneAnswer - m_phoneManufacturer - m_phoneModel - m_phoneBattery - m_phoneRevision - m_phoneStatus - m_defaultBtDevice - m_defaultIrdaDevice - m_defaultSerialDevice - m_settingsAll - m_settingsDevice - m_settingsBtAddress - m_settingsConnectStartup - m_settingsBtChannel - m_phoneContactEntry - m_phoneContactId - m_phoneContactType - m_phoneContactName - m_phoneContactNumber - m_phoneContactCount - m_phoneSmsEntry - m_phoneSmsId - m_phoneSmsStatus - m_phoneSmsDateTmp - m_phoneSmsDate - m_phoneSmsNumber - m_phoneSmsMessage - m_phoneSmsToShow - m_PDU - m_PduLength - m_index - m_id - m_AtCommand - m_FileName - m_UploadFileName - m_UploadFilePath

+ BluePhone() + ~BluePhone() + readSettings() + setSettingsView() + showMetaInfo() + settingsSave + settingsGetAddress + contactsSms + contactsCall + contactsRestore + contactsBackup + contactsDelete + contactsEdit + contactsNew + contactsRead + smsNew + smsDeleteAll + smsDelete + smsSaveAll + smsSave + smsRead + smsShow + smsReply + fileSend + fileBrowse + phoneGetInfo + phoneDisconnect + phoneConnect + helpAbout + fileExit + setLedGreen + setLedOrange + setLedRed + sendContactToPhone + sendSmsToPhone

FormBluePhone

QString

m_UploadFileName m_settingsAll m_phoneContactType m_defaultBtDevice m_FileName m_phoneSmsNumber m_phoneSmsStatus m_phoneContactId m_BtChannel m_phoneSmsEntry m_phoneStatus m_phoneSmsMessage m_phoneManufacturer m_phoneSmsDateTmp m_phoneContactCount m_PDU m_phoneSmsDate m_phoneSmsId m_ConnectStartup version m_PduLength m_defaultIrdaDevice m_phoneRevision m_phoneContactNumber m_settingsBtAddress m_phoneBattery m_Device m_phoneContactEntry m_settingsDevice m_BtAddress m_UploadFilePath m_AtCommand m_phoneSmsToShow m_phoneContactName m_settingsConnectStartup m_defaultSerialDevice m_phoneModel

BlueLink

- m_communicate - m_connected - m_port - m_phoneAnswer - m_phoneMode - m_rfcommCommand

+ BlueLink() + ~BlueLink() + connectRfcomm() + disconnectRfcomm() + connecttoPhone() + getPort() + getState() + disconnectPhone() + talktoPhone() m_rfcommCommand m_phoneMode

BlueConvert

- m_PDU - m_sender - m_message - m_date - m_posInPdu - m_smscType - m_smscLen - m_senderLength - m_senderType - m_udhLength - m_rp - m_rplength - m_ie - m_messageLength - m_swapped - m_recipient - m_index - m_id - m_longMessage - m_recipientType - m_recipientLength - m_recipientLengthHex - m_carryoverLength - m_encodedMessage

+ BlueConvert() + ~BlueConvert() + convert_from_gsm() + convert_to_gsm() + decodeMessage() + encodeMessage() + extractPduData() + createPduData() + decodeBCD() + getSender() + getDate() + getMessage() + getPdu() m_swapped m_date m_message m_sender m_recipientLengthHex m_carryoverLength m_recipientType m_PDU m_recipient m_senderType m_encodedMessage v24_port_t *

m_Port m_port int

m_index m_BtChannelInt m_id m_settingsBtChannel m_index m_smscType m_rp m_posInPdu m_senderLength m_messageLength m_rplength m_longMessage m_udhLength m_recipientLength m_id m_ie m_smscLen

myLink

QStringList

m_phoneAnswer m_phoneAnswer

myConvert